R 535
Flow over trails with increased small bump sensitivity.
The R 535 All Mountain shock has been modified at its air chambers; the displacement of the bypass allows the chambers to change their volumes, which will lead to better small bump compliance, in order to flow over trails while still having sufficient mid-stroke support and firm end progression. Equipped with a lever, the shock can be locked and unlocked to adapt to the needs that arise on the trails.